⚠
AMSpiriT is not connected.
Please start the emulator with the web server enabled
Waiting for connection…

# AMSpiriT — Web Interface

Language
Running FPS: --.- Frame: --.- ms Model: -- CRTC: --

## Virtual Keyboard

## CPC Keyboard Matrix — `G_CORE_BKeyState_CPC`

## BASIC program

## Variables

TXTTOP ---- Size ---- Vars zone ---- Arrays zone ---- Free RAM ---- Stmt addr ---- Version ----

Name | Type | Value
--- | --- | ---

No variables
Arrays

Name | Dims | Values
--- | --- | ---

Address

## Z80

## Circuits

Bank:
Search (hex):

    —

buffer en cours buffer complet zone visible

## Disassembler
Follow PC

No data — press Refresh.

## Last instructions

--
Window:
Device:
Volume: 100%

## PSG AY-3-8912

## Spectrum (FFT)

## Spectrogramme (FFT) Durée :

— ← temps maintenant

## RAM — Write Heatmap

Mode
Decay
Overlay: PC SP HL IX IY RAM bg
Bank:
C0:0000 C1:0000 C2:0000 C3:0000 C3:3FFF
xx00 xx40 xx80 xxC0 xxFF
1 pixel = 1 byte
Y = high byte of address
X = low byte of address
cold hot
● PC ● SP ● HL ● IX ● IY
overlay on C0 only
0 RAM bg 255

## RAM — Write / Load

Bank:
Write address Entry point (exec) Data (hex)
Hex data may contain spaces, colons, etc.

## Script CSL / Lua

## Configuration

CPC Model
CRTC Type
(resets the emulator)

## Display & CRT

Monitor
Screen type

Selecting a monitor loads its defaults; tweak the sliders for a live preview.

## CRT shader parameters

Monitor is Off — the CRT shader is bypassed, so these settings have no effect.

## Drive A

## Drive B

## Keyboard Mapping ▼